AD-4405/06/07 UFC Command

Format
 SF1,[parameters]     Set serial output format1 (F34)
 SF2,[parameters]     Set serial output format2 (F35)
 PF1,[parameters]     Set print out format1 (F70)  for AD-4405 
 PF2,[parameters]     Set print out format2 (F71)  for AD-4405 

Parameter
 $xx    Indicator's data (nit only weight)   ex. $WT, $DT
 'xxx'  Text (expression in ASCII code)      ex. 'A & D Co., Ltd.'
 #00    Character in hex-decimal             ex. #1E, #0C
 
 Multi parameters can use in one command line without any delimitter.
   ex.  SF1,$DT$CM$WT'abcd'#0D$LF

Data
 $ID    Unit number or ID, this parameter is set by F06
 $DT    Date (AD-4405)
 $TM    Time (AD-4405)
 $DN    Data number, increments automatically after output
 $CD    Code number

 $WT    Displayed weight data
 $GR	Gross weight
 $NT    Net weight
 $TR    Tare weight
 $PT    Preset tare weight (AD-4405/07)
 $PC    Piece count (AD-4405/07)
 $UW    Unit weight for piece counting (AD-4405/07)
 $HD    Gross, net, tare or preset tare
 $UT	Unit of weight
 $ST    Status (stable or no)
 $CP    Result of comparison (HH, HI, OK, LO, LL)
 $AN    Number of accumulation
 $TL	Total(accumulated) weight

 $CM    Comma
 $CR    Carriage return code (0Dh)
 $LF    Line feed code (0Ah)
 $CL    Clear the former setting
 $DE    Delete last entried command line
 $DL    Insert delay time (00-99:0.0s to 9.9s)

Text
 'text'   ' itself : ''

#
 For control code of the printer etc.

